{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["GB","ES","FR","CZ","DE","IT","MX-PT","NL","TR"],"not_rendered":{"charts":27,"images":2,"macros":1,"external_links":0,"defined_names":9,"comments":9,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"GB","index":0,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[2,17,2,19],[10,5,12,5],[10,6,12,6],[10,7,12,7],[10,8,12,8],[13,5,15,5],[13,6,15,6],[13,7,15,7],[13,8,15,8],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[13,0,15,0],[13,1,15,1],[13,2,15,2],[13,3,15,3],[13,4,15,4],[16,6,18,6],[16,7,18,7],[16,8,18,8],[25,7,27,7],[9,15,22,21],[24,15,37,21],[25,8,27,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[28,6,30,6],[28,7,30,7],[16,5,18,5],[28,8,30,8],[31,5,33,5],[9,9,22,14],[25,0,27,0],[25,1,27,1],[25,2,27,2],[25,3,27,3],[28,3,30,3],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,4,30,4],[25,4,27,4],[25,5,27,5],[25,6,27,6],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[53,0,53,21],[6,4,6,5],[6,7,6,8],[39,9,41,14],[43,2,52,14],[7,17,7,19],[6,16,6,19],[39,15,52,21],[7,0,7,3],[7,4,7,7],[7,8,7,9],[7,10,7,11],[7,12,7,13],[7,14,7,15],[24,9,37,14],[28,5,30,5]]}
["Enable macros with the options button first!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["FUEL INJECTOR DIAGNOSTIC TEST & SERVICE REPORT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["ASNU Injector Service Centre : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tel : "]
["Customer name : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email : "]
["Address : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date : "]
["Vehicle Make / Reference : ",null,null,null,null,null,"/",null,null,"Model : ",null,null,"Year : ",null,null,null,"Serviced by :"]
["Injector type : ",null,null,null,null,null,null,null,"Part number : ",null,null,null,"Test pressure : "]
["Test A (before cleaning)",null,null,null,null,null,null,null,null,"Photos",null,null,null,null,null,"Flow (cc)"]
[null,1,2,3,4,5,6,7,8]
["Leak test pass"]
[]
[]
["Spray pattern"]
[]
[]
["Auto mS/rpm sweep"]
[]
[]
["Inductance (mH)"]
["FLOW SETTINGS","mS",null,"RPM",null,"Time",null,"Time"]
["Flow (dynamic)"]
["Flow (static)"]
["Test B (after cleaning)",null,null,null,null,null,null,null,null,"Photos",null,null,null,null,null,"Flow (cc)"]
[null,1,2,3,4,5,6,7,8]
["Leak test"]
[]
[]
["Spray pattern"]
[]
[]
["Auto mS/rpm sweep"]
[]
[]
["Inductance (mH)"]
["FLOW SETTINGS","mS",{"$f":"C21","v":0},"RPM",{"$f":"E21","v":0},"Time",{"$f":"G21","v":0},"Time",{"$f":"I21","v":0}]
["Flow (dynamic)"]
["Flow (static)"]
["Flow change (%)                                                            ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Flow change (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Flow (dynamic)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Flow (static)","","","","","","","",""]
["Parts used                                                           ",null,"Comments & recommendations"]
["Pintel caps"]
["O-ring (top)"]
["O-ring (bottom)"]
["Filter baskets"]
["Spacers"]
["Teflon seals"]
["Rubber seals"]
["Rubber pipe"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"ES","index":1,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["¡Habilite las macros con el botón de opciones primero!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["Datos de prueba",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["Centro de servicio ASNU : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tel : "]
["Nombre cliente : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email : "]
["Dirección : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fecha : "]
["Marca vehículo / Referencia : ",null,null,null,null,null,"/",null,null,"Modelo : ",null,null,"Año : ",null,null,null,"Atendido por :"]
["Tipo inyector : ",null,null,null,null,null,null,null,"Número de serie : ",null,null,null,"Presión de prueba : "]
["Prueba A (antes de limpiar)",null,null,null,null,null,null,null,null,"Fotos",null,null,null,null,null,"Flujo (cc)"]
[null,1,2,3,4,5,6,7,8]
["Prueba de\nfugas"]
[]
[]
["Pulverizado"]
[]
[]
["Barrido automático mS/rpm"]
[]
[]
["Inductancia (mH)"]
["CONFIGURACIÓN DE FLUJO","mS:",null,"RPM:",null,"Hora",null,"Hora"]
["Flujo (dinámico)"]
["Flujo (estático)"]
["Prueba B (después de la limpieza)",null,null,null,null,null,null,null,null,"Fotos",null,null,null,null,null,"Flujo (cc)"]
[null,1,2,3,4,5,6,7,8]
["Prueba de\nfugas"]
[]
[]
["Pulverizado"]
[]
[]
["Barrido automático mS/rpm"]
[]
[]
["Inductancia (mH)"]
["CONFIGURACIÓN DE FLUJO","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Hora",{"$f":"G21","v":0},"Hora",{"$f":"I21","v":0}]
["Flujo (dinámico)"]
["Flujo (estático)"]
["Cambio flujo (%)             ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cambio flujo (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Flujo (dinámico)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Flujo (estático)","","","","","","","",""]
["Recambios:                                    ",null,"Comentarios & recomendaciones"]
["Copela"]
["Anillo tórico superior"]
["Anillo tórico inferior"]
["Micro filtro"]
["Espaciadores"]
["Sellos de teflón"]
["Junta de goma"]
["Tubería de goma"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"FR","index":2,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["Activer les macros avec le bouton Options en premier!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["FICHE DE RAPPORT D’ESSAID'INJECTEURSESSENCE",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["Centre Technique :\n ASNU \n : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tel : "]
["Nom du client : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email : "]
["Adresse : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Date : "]
["Marque du véhicule / Référence : ",null,null,null,null,null,"/",null,null,"Modèle : ",null,null,"Année : ",null,null,null,"Technicien :"]
["Type d’injecteur : ",null,null,null,null,null,null,null,"Référence : ",null,null,null,"Test pression  : "]
["Test A (Avant le nettoyage)",null,null,null,null,null,null,null,null,"Photos",null,null,null,null,null,"Flow (cc)"]
[null,1,2,3,4,5,6,7,8]
["Test de fuite"]
[]
[]
["Forme des jets"]
[]
[]
["Mode automatique mS / rpm"]
[]
[]
["Inductance (mH)"]
["REGLAGES DE FLOW","mS:",null,"RPM:",null,"Temps",null,"Temps"]
["Flow (dynamique)"]
["Flow (statique)"]
["Test B (Après le nettoyage)",null,null,null,null,null,null,null,null,"Photos",null,null,null,null,null,"Flow (cc)"]
[null,1,2,3,4,5,6,7,8]
["Test de fuite"]
[]
[]
["Forme des jets"]
[]
[]
["Mode automatique mS / rpm"]
[]
[]
["Inductance (mH)"]
["REGLAGES DE FLOW","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Temps",{"$f":"G21","v":0},"Temps",{"$f":"I21","v":0}]
["Flow (dynamique)"]
["Flow (statique)"]
["Changement de débit (%)                                                 ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Changement de débit (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Flow (dynamique)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Flow (statique)","","","","","","","",""]
["Pièces remplacées                                            ",null,"Commentaires et recommandations"]
["Capuchons"]
["Joint torique (haut)"]
["Joint torique (bas)"]
["Filtres"]
["Spacers"]
["Joints en téflon"]
["Joints en caoutchouc"]
["Tuyau en caoutchouc "]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"CZ","index":3,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["Aktivujte nejdříve makra pomocí tlačítka možností."]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["ZKOUŠKA DIAGNOSTICKÉHO ZKOUŠKY A SERVIS ZAŘÍZENÍ PALIVA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["Servisní středisko ASNU Injector :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telefon : "]
["Jméno zákazníka :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E-mailem "]
["Adresa :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Datum : "]
["Značka vozidla / Odkaz :",null,null,null,null,null,"/",null,null,"Modelka :",null,null,"Rok :",null,null,null,"Servisováno :"]
["Typ vstřikovače :",null,null,null,null,null,null,null,"Objednací číslo :",null,null,null,"Zkušební tlak :"]
["Test A (před čištěním)",null,null,null,null,null,null,null,null,"Fotografie",null,null,null,null,null,"Tok (cc)"]
[null,1,2,3,4,5,6,7,8]
["Průběh zkoušky\n těsnosti"]
[]
[]
["Vzorek\n postřiku"]
[]
[]
["Automatické mS / otáčky za minutu"]
[]
[]
["Indukčnost (mH)"]
["NASTAVENÍ TOK","mS:",null,"RPM:",null,"Čas",null,"Čas"]
["Tok (dynamický)"]
["Průtok (statický)"]
["Test B (po čištění)",null,null,null,null,null,null,null,null,"Fotografie",null,null,null,null,null,"Tok (cc)"]
[null,1,2,3,4,5,6,7,8]
["Průběh zkoušky\n těsnosti"]
[]
[]
["Vzorek\n postřiku"]
[]
[]
["Automatické mS / otáčky za minutu"]
[]
[]
["Indukčnost (mH)"]
["NASTAVENÍ TOK","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Čas",{"$f":"G21","v":0},"Čas",{"$f":"I21","v":0}]
["Tok (dynamický)"]
["Průtok (statický)"]
["Změna průtoku (%)                                                    ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Změna průtoku (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Tok (dynamický)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Průtok (statický)","","","","","","","",""]
["Použité díly                                                  ",null,"Komentáře a doporučení"]
["Pytlové čepičky"]
["O-kroužek (horní)"]
["O-kroužek (spodní)"]
["Filtrační koše"]
["Rozdělovače"]
["Teflonové těsnění"]
["Gumové těsnění"]
["Gumová trubka"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"DE","index":4,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["Aktivieren Sie Makros mit dem Optionsfeld zuerst!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["KRAFTSTOFFINJEKTOR DIAGNOSTIC TEST & SERVICE REPORT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["ASNU Injector Service Center : ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telefon :"]
["Kundenname :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email : "]
["Adresse :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Datum :"]
["Automarke / Referenz :",null,null,null,null,null,"/",null,null,"Modell :",null,null,"Jahr :",null,null,null,"Bewirtschaftet von :"]
["Injektortyp :",null,null,null,null,null,null,null,"Artikelnummer :",null,null,null,"Prüfungsangst :"]
["Test A (vor der Reinigung)",null,null,null,null,null,null,null,null,"Fotos",null,null,null,null,null,"Fluss (cc)"]
[null,1,2,3,4,5,6,7,8]
["Lecktest bestanden"]
[]
[]
["Sprühmuster"]
[]
[]
["Auto mS / U / Min"]
[]
[]
["Induktivität (mH)"]
["FLUSSEINSTELLUNGEN","mS:",null,"RPM:",null,"Zeit",null,"Zeit"]
["Fluss (dynamisch)"]
["Fluss (statisch)"]
["Test B (nach der Reinigung)",null,null,null,null,null,null,null,null,"Fotos",null,null,null,null,null,"Fluss (cc)"]
[null,1,2,3,4,5,6,7,8]
["Lecktest bestanden"]
[]
[]
["Sprühmuster"]
[]
[]
["Auto mS / U / Min"]
[]
[]
["Induktivität (mH)"]
["FLUSSEINSTELLUNGEN","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Zeit",{"$f":"G21","v":0},"Zeit",{"$f":"I21","v":0}]
["Fluss (dynamisch)"]
["Fluss (statisch)"]
["Durchflussänderung (%)                                                            ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Durchflussänderung (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Fluss (dynamisch)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Fluss (statisch)","","","","","","","",""]
["Teile verwendet                                    ",null,"Kommentare und Empfehlungen"]
["Zapfenkappen"]
["O-Ring (oben)"]
["O-Ring (unten)"]
["Filterkörbe"]
["Abstandshalter"]
["Teflon Dichtungen"]
["Gummidichtungen"]
["Gummirohr"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"IT","index":5,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["Abilita le macro con il pulsante opzioni prima!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["TEST DIAGNOSTICO INIETTORE CARBURANTE E RAPPORTO DI ASSISTENZA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["Centro di assistenza iniettori ASNU :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telefono"]
["Nome del cliente :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E-mail :"]
["Indirizzo :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Data :"]
["Marca del veicolo / Riferimento :",null,null,null,null,null,"/",null,null,"Modello :",null,null,"Anno :",null,null,null,"Servito da :"]
["Tipo di iniettore :",null,null,null,null,null,null,null,"Numero di parte :",null,null,null,"Pressione di prova :"]
["Test A (prima della pulizia)",null,null,null,null,null,null,null,null,"Foto",null,null,null,null,null,"Flusso (cc)"]
[null,1,2,3,4,5,6,7,8]
["Prova di tenuta"]
[]
[]
["Modello di spruzzo"]
[]
[]
["Auto mS/rpm spazzare"]
[]
[]
["Induttanza (mH)"]
["IMPOSTAZIONI DI FLUSSO","mS:",null,"RPM:",null,"Tempo",null,"Tempo"]
["Flusso (dinamico)"]
["Flusso (statico)"]
["Test B (dopo la pulizia)",null,null,null,null,null,null,null,null,"Foto",null,null,null,null,null,"Flusso (cc)"]
[null,1,2,3,4,5,6,7,8]
["Prova di tenuta"]
[]
[]
["Modello di spruzzo"]
[]
[]
["Auto mS/rpm spazzare"]
[]
[]
["Induttanza (mH)"]
["IMPOSTAZIONI DI FLUSSO","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Tempo",{"$f":"G21","v":0},"Tempo",{"$f":"I21","v":0}]
["Flusso (dinamico)"]
["Flusso (statico)"]
["Flow change (%)                                                            ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Flow change (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Flusso (dinamico)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Flusso (statico)","","","","","","","",""]
["Parti utilizzate                                                 ",null,"Commenti e raccomandazioni"]
["Cappucci a punta"]
["O-ring (in alto)"]
["O-ring (in basso)"]
["Cesti filtranti"]
["Distanziatori"]
["Guarnizioni in teflon"]
["Guarnizioni di gomma"]
["Tubo di gomma"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"MX-PT","index":6,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["Ativar macros com o botão de opções primeiro!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["TESTE DE DIAGNÓSTICO DO INJETOR DE COMBUSTÍVEL E RELATÓRIO DE SERVIÇO",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["Centro de Serviço de Injetor ASNU :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telefone"]
["Nome do cliente :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Email"]
["Endereço :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Encontro "]
["Veículo fazer / Referência :",null,null,null,null,null,"/",null,null,"Modelo :",null,null,"Ano :",null,null,null,"Servido por :"]
["Tipo de injetor :",null,null,null,null,null,null,null,"Número da peça :",null,null,null,"Pressão de teste :"]
["Teste A (antes de limpar)",null,null,null,null,null,null,null,null,"Fotos",null,null,null,null,null,"Fluxo (cc)"]
[null,1,2,3,4,5,6,7,8]
["Teste de vazamento"]
[]
[]
["Padrão de pulverização"]
[]
[]
["Varredura automática de mS / rpm"]
[]
[]
["Indutância (mH)"]
["CONFIGURAÇÕES DE FLUXO","mS:",null,"RPM:",null,"Tempo",null,"Tempo"]
["Fluxo (dinâmico)"]
["Fluxo (estático)"]
["Teste B (após a limpeza)",null,null,null,null,null,null,null,null,"Fotos",null,null,null,null,null,"Fluxo (cc)"]
[null,1,2,3,4,5,6,7,8]
["Teste de vazamento"]
[]
[]
["Padrão de pulverização"]
[]
[]
["Varredura automática de mS / rpm"]
[]
[]
["Indutância (mH)"]
["CONFIGURAÇÕES DE FLUXO","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Tempo",{"$f":"G21","v":0},"Tempo",{"$f":"I21","v":0}]
["Fluxo (dinâmico)"]
["Fluxo (estático)"]
["Flow change (%)                                                            ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Flow change (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Fluxo (dinâmico)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Fluxo (estático)","","","","","","","",""]
["Peças usadas                                            ",null,"Comentários e recomendações"]
["Tampas de pintle"]
["O-ring (superior)"]
["O-ring (inferior)"]
["Cestas de filtro"]
["Espaçadores"]
["Vedações de teflon"]
["Vedações de borracha"]
["Cano de borracha"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"NL","index":7,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["Schakel eerst macro's in met de optieknop!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["Injector diagnose test en servicerapport",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["ASNU Injector Service Center :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telefoon"]
["Klantnaam :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E-mail : "]
["Adres :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Datum :"]
["Voertuig merk / Referentie :",null,null,null,null,null,"/",null,null,"Model : ",null,null,"Jaar :",null,null,null,"Beheerd door :"]
["Injector type : ",null,null,null,null,null,null,null,"Onderdeel nummer",null,null,null,"Test druk :"]
["Test A (voor reinigen)",null,null,null,null,null,null,null,null,"Foto's",null,null,null,null,null,"Flow (cc)"]
[null,1,2,3,4,5,6,7,8]
["Lektest geslaagd"]
[]
[]
["Sproeipatroon"]
[]
[]
["Auto ms/rpm test"]
[]
[]
["Inductie (mH)"]
["FLOW-INSTELLINGEN","mS:",null,"RPM:",null,"Tijd",null,"Tijd"]
["Flow (dynamisch)"]
["Flow (statisch)"]
["Test B (na reinigen)",null,null,null,null,null,null,null,null,"Foto's",null,null,null,null,null,"Flow (cc)"]
[null,1,2,3,4,5,6,7,8]
["Lektest geslaagd"]
[]
[]
["Sproeipatroon"]
[]
[]
["Auto ms/rpm test"]
[]
[]
["Inductie (mH)"]
["FLOW-INSTELLINGEN","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Tijd",{"$f":"G21","v":0},"Tijd",{"$f":"I21","v":0}]
["Flow (dynamisch)"]
["Flow (statisch)"]
["Flow change (%)                                                            ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Flow verschil (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Flow (dynamisch)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Flow (statisch)","","","","","","","",""]
["Gebruikte onderdelen                                 ",null,"Opmerkingen en aanbevelingen"]
["Pintle caps"]
["O-ring (boven)"]
["O-ring (onder)"]
["Filters"]
["Vulringen"]
["Teflon afdichtingen"]
["Rubberen afdichtingen"]
["Rubberen slang"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]

{"sheet":"TR","index":8,"n_rows":55,"n_cols":22,"rows_kept":55,"cut":false,"hidden":false,"merged":[[0,0,0,21],[2,17,2,19],[2,20,6,21],[3,0,3,3],[3,4,3,15],[3,17,3,19],[4,0,4,3],[4,4,4,15],[4,17,4,19],[5,0,5,3],[5,4,5,15],[5,17,5,19],[6,0,6,3],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,19],[7,17,7,19],[9,9,22,14],[9,15,22,21],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,8,7,9],[13,8,15,8],[10,8,12,8],[10,5,12,5],[10,6,12,6],[7,0,7,3],[7,4,7,7],[13,5,15,5],[13,6,15,6],[13,7,15,7],[10,7,12,7],[10,0,12,0],[10,1,12,1],[10,2,12,2],[10,3,12,3],[10,4,12,4],[16,7,18,7],[16,8,18,8],[13,0,15,0],[13,1,15,1],[13,2,15,2],[16,0,18,0],[16,1,18,1],[16,2,18,2],[16,3,18,3],[16,4,18,4],[13,3,15,3],[13,4,15,4],[25,2,27,2],[25,3,27,3],[25,4,27,4],[16,5,18,5],[16,6,18,6],[28,7,30,7],[28,8,30,8],[25,5,27,5],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[25,8,27,8],[28,0,30,0],[28,1,30,1],[28,2,30,2],[28,3,30,3],[28,4,30,4],[25,0,27,0],[25,1,27,1],[53,0,53,21],[6,4,6,5],[6,7,6,8],[31,6,33,6],[31,7,33,7],[31,8,33,8],[39,9,41,14],[39,15,52,21],[43,2,52,14],[31,5,33,5],[24,9,37,14],[24,15,37,21],[25,6,27,6],[25,7,27,7],[28,5,30,5],[28,6,30,6]]}
["Önce seçenekler düğmesiyle makroları etkinleştirin!"]
[{"$f":"REPLACE(LEFT(CELL(\"filename\",A2),FIND(\"]\",CELL(\"filename\",A2))-1),1,FIND(\"[\",CELL(\"filename\",A2)),\"\")","v":"ASNU Interactive Report Sheet.xlsm"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version : ",19.510000000000002]
["YAKIT ENJEKTÖRÜNÜN TANI VE HİZMET RAPORU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"www.asnu.com"]
["ASNU Enjektör Servis Merkezi :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Telefon"]
["Müşteri adı :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E-posta"]
["Adres :",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tarih : "]
["Araç yapmak / Referans :",null,null,null,null,null,"/",null,null,"Model : ",null,null,"Yıl :",null,null,null,"Hizmet veren :"]
["Enjektör tipi :",null,null,null,null,null,null,null,"Parça numarası :",null,null,null,"Test basıncı :"]
["Test A (temizlemeden önce)",null,null,null,null,null,null,null,null,"Fotoğraf",null,null,null,null,null,"Akış (cc)"]
[null,1,2,3,4,5,6,7,8]
["Sızıntı testi geçmek"]
[]
[]
["Püskürtme şekli"]
[]
[]
["Otomatik mS / rpm süpürme"]
[]
[]
["Endüktans (mH)"]
["AKIŞ AYARLARI","mS:",null,"RPM:",null,"Zaman",null,"Zaman"]
["Akış (dinamik)"]
["Akış (statik)"]
["Test B (temizlendikten sonra)",null,null,null,null,null,null,null,null,"Fotoğraf",null,null,null,null,null,"Akış (cc)"]
[null,1,2,3,4,5,6,7,8]
["Sızıntı testi geçmek"]
[]
[]
["Püskürtme şekli"]
[]
[]
["Otomatik mS / rpm süpürme"]
[]
[]
["Endüktans (mH)"]
["AKIŞ AYARLARI","mS:",{"$f":"C21","v":0},"RPM:",{"$f":"E21","v":0},"Zaman",{"$f":"G21","v":0},"Zaman",{"$f":"I21","v":0}]
["Akış (dinamik)"]
["Akış (statik)"]
["Flow change (%)                                                            ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Flow change (%)"]
[null,1,2,3,4,5,6,7,8,"www.asnu.com"]
["Akış (dinamik)",{"$f":"IF(OR(ISBLANK(B22),ISBLANK(B37)),\"\",((B37-B22)/B22)*100)","v":""},"","","","","","",""]
["Akış (statik)","","","","","","","",""]
["Kullanılan parçalar                                                  ",null,"Yorumlar ve öneriler"]
["Pintle başlıkları"]
["O-ring (üst)"]
["O-ring (alt)"]
["Filtre sepetleri"]
["Paspayı"]
["Teflon mühürler"]
["Kauçuk contalar"]
["Kauçuk boru"]
[]
[]
[]
["Copyright : PHAB Design Ltd"]